a. Use the USB cable to connect the keyboard and computer normally;

b. Double-click the firmware, wait for the progress bar to finish automatically, and then re-plug the USB cable to take effect.